Міністерство освіти і науки України

Національний університет «Львівська політехніка»

Кафедра ЕОМ



Звіт

до лабораторної роботи № 3

з дисципліни «Моделювання комп’ютерних систем»

на тему:

«Поведінковий опис цифрового автомата Перевірка роботи автомата за допомогою стенда Elbert V2 – Spartan 3A FPGA»

Варіант №1

Виконав:

ст. гр. КІ-201

Бандрівський П.Р


Прийняв:

ст. викладач   
каф. ЕОМ  
Козак Н. Б.

Львів 2024

**Мета роботи**: На базі стенда реалізувати цифровий автомат для обчислення значення виразів.

**Виконання роботи:**

****

*Рис. 1 – Top Level*

|  |
| --- |
| Файл ACC.vhd  *library IEEE;*  *use IEEE.STD\_LOGIC\_1164.ALL;*  *use IEEE.STD\_LOGIC\_ARITH.ALL;*  *use IEEE.STD\_LOGIC\_UNSIGNED.ALL;*  *entity ACC is*  *Port ( WR : in STD\_LOGIC;*  *RST : in STD\_LOGIC;*  *CLK : in STD\_LOGIC;*  *IN\_BUS : in STD\_LOGIC\_VECTOR (7 downto 0);*  *OUT\_BUS : out STD\_LOGIC\_VECTOR (7 downto 0));*  *end ACC;*  *architecture ACC\_arch of ACC is*  *signal DATA : STD\_LOGIC\_VECTOR (7 downto 0);*  *begin*  *process (CLK)*  *begin*  *if rising\_edge(CLK) then*  *if RST = '1' then*  *DATA <= (others => '0');*  *elsif WR = '1' then*  *DATA <= IN\_BUS;*  *end if;*  *end if;*  *end process;*    *OUT\_BUS <= DATA;*  *end ACC\_arch;* |


|  |
| --- |
| Файл ALU.vhd  library IEEE;  use IEEE.STD\_LOGIC\_1164.ALL;  use IEEE.STD\_LOGIC\_UNSIGNED.ALL;  use ieee.NUMERIC\_STD.all;  entity ALU is  Port (  A, B : in STD\_LOGIC\_VECTOR(7 downto 0);  ALU\_Sel : in STD\_LOGIC\_VECTOR(1 downto 0);  ALU\_Out : out STD\_LOGIC\_VECTOR(7 downto 0);  Carryout : out std\_logic  );  end ALU;  architecture Behavioral of ALU is  signal ALU\_Result : std\_logic\_vector (8 downto 0);  begin  process(A,B,ALU\_Sel)  begin  case(ALU\_Sel) is  when "01" =>  ALU\_Result <= ('0' & A) + ('0' & B);  when "10" =>  ALU\_Result <= ('0' & A) and ('0' & B);  when "11" =>  case(B) is  when x"00" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 0);  when x"01" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 1);  when x"02" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 2);  when x"03" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 3);  when x"04" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 4);  when x"05" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 5);  when x"06" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 6);  when x"07" => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 7);  when others => ALU\_Result <= std\_logic\_vector(unsigned(('0' & A)) sll 0);  end case;  ALU\_Result(8) <= '0';  when others => ALU\_Result <= ('0' & B);  end case;  end process;  ALU\_Out <= ALU\_Result(7 downto 0);  Carryout <= ALU\_Result(8);  end Behavioral; |

|  |
| --- |
| Файл CPU.vhd  library IEEE;  use IEEE.STD\_LOGIC\_1164.ALL;  entity CU is  port( ENTER\_OP1 : IN STD\_LOGIC;  ENTER\_OP2 : IN STD\_LOGIC;  CALCULATE : IN STD\_LOGIC;  RESET : IN STD\_LOGIC;  CLOCK : IN STD\_LOGIC;  RAM\_WR : OUT STD\_LOGIC;  RAM\_ADDR\_BUS : OUT STD\_LOGIC\_VECTOR(1 DOWNTO 0);  CONST\_BUS : OUT STD\_LOGIC\_VECTOR(7 DOWNTO 0);  ACC\_WR : OUT STD\_LOGIC;  ACC\_RST : OUT STD\_LOGIC;  MUX\_SEL\_BUS : OUT STD\_LOGIC\_VECTOR(1 DOWNTO 0);  OP\_CODE\_BUS : OUT STD\_LOGIC\_VECTOR(1 DOWNTO 0));  end CU;    architecture CU\_arch of CU is  type STATE\_TYPE is (RST, IDLE, LOAD\_OP1, LOAD\_OP2, RUN\_CALC0, RUN\_CALC1, RUN\_CALC2, RUN\_CALC3, RUN\_CALC4, FINISH);  signal CUR\_STATE : STATE\_TYPE;  signal NEXT\_STATE : STATE\_TYPE;  begin  CONST\_BUS <= "00001010";      SYNC\_PROC: process (CLOCK)  begin  if (rising\_edge(CLOCK)) then  if (RESET = '1') then  CUR\_STATE <= RST;  else  CUR\_STATE <= NEXT\_STATE;  end if;  end if;  end process;      NEXT\_STATE\_DECODE: process (CUR\_STATE, ENTER\_OP1, ENTER\_OP2, CALCULATE)  begin  --declare default state for next\_state to avoid latches  NEXT\_STATE <= CUR\_STATE; --default is to stay in current state  --insert statements to decode next\_state  --below is a simple example  case(CUR\_STATE) is  when RST =>  NEXT\_STATE <= IDLE;  when IDLE =>  if (ENTER\_OP1 = '1') then  NEXT\_STATE <= LOAD\_OP1;  elsif (ENTER\_OP2 = '1') then  NEXT\_STATE <= LOAD\_OP2;  elsif (CALCULATE = '1') then  NEXT\_STATE <= RUN\_CALC0;  else  NEXT\_STATE <= IDLE;  end if;  when LOAD\_OP1 =>  NEXT\_STATE <= IDLE;  when LOAD\_OP2 =>  NEXT\_STATE <= IDLE;  when RUN\_CALC0 =>  NEXT\_STATE <= RUN\_CALC1;  when RUN\_CALC1 =>  NEXT\_STATE <= RUN\_CALC2;  when RUN\_CALC2 =>  NEXT\_STATE <= RUN\_CALC3;  when RUN\_CALC3 =>  NEXT\_STATE <= RUN\_CALC4;  when RUN\_CALC4 =>  NEXT\_STATE <= FINISH;  when FINISH =>  NEXT\_STATE <= FINISH;  when others =>  NEXT\_STATE <= IDLE;  end case;  end process;  OUTPUT\_DECODE: process (CUR\_STATE)  begin  case(CUR\_STATE) is  when RST =>  MUX\_SEL\_BUS <= "00";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '1';  ACC\_WR <= '0';  when IDLE =>  MUX\_SEL\_BUS <= "00";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '0';  when LOAD\_OP1 =>  MUX\_SEL\_BUS <= "00";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '1';  ACC\_RST <= '0';  ACC\_WR <= '1';  when LOAD\_OP2 =>  MUX\_SEL\_BUS <= "00";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "01";  RAM\_WR <= '1';  ACC\_RST <= '0';  ACC\_WR <= '1';  when RUN\_CALC0 =>  MUX\_SEL\_BUS <= "01";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '1';  when RUN\_CALC1 =>  MUX\_SEL\_BUS <= "01";  OP\_CODE\_BUS <= "01";  RAM\_ADDR\_BUS <= "01";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '1';  when RUN\_CALC2 =>  MUX\_SEL\_BUS <= "11";  OP\_CODE\_BUS <= "01";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '1';  when RUN\_CALC3 =>  MUX\_SEL\_BUS <= "01";  OP\_CODE\_BUS <= "10";  RAM\_ADDR\_BUS <= "01";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '1';  when RUN\_CALC4 =>  MUX\_SEL\_BUS <= "01";  OP\_CODE\_BUS <= "11";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '1';  when FINISH =>  MUX\_SEL\_BUS <= "00";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '0';  when others =>  MUX\_SEL\_BUS <= "00";  OP\_CODE\_BUS <= "00";  RAM\_ADDR\_BUS <= "00";  RAM\_WR <= '0';  ACC\_RST <= '0';  ACC\_WR <= '0';  end case;  end process;  end CU\_arch; |


|  |
| --- |
| Файл MUX.vhd  library IEEE;  use IEEE.STD\_LOGIC\_1164.ALL;  entity MUX is  Port ( SEL : in STD\_LOGIC\_VECTOR (1 downto 0);  CONST : in STD\_LOGIC\_VECTOR (7 downto 0);  RAM\_DATA\_OUT : in STD\_LOGIC\_VECTOR (7 downto 0);  DATA\_IN : in STD\_LOGIC\_VECTOR (7 downto 0);  O : out STD\_LOGIC\_VECTOR (7 downto 0));  end MUX;  architecture MUX\_arch of MUX is  begin    PROCESS (SEL, CONST, RAM\_DATA\_OUT, DATA\_IN)  BEGIN  IF (SEL = "00") THEN  O <= DATA\_IN;  ELSIF (SEL = "01") THEN  O <= RAM\_DATA\_OUT;  ELSE  O <= CONST;  END IF;  END PROCESS;  end MUX\_arch; |

|  |
| --- |
| Файл RAM.vhd  library IEEE;  use IEEE.STD\_LOGIC\_1164.ALL;  use IEEE.NUMERIC\_STD.ALL;  use IEEE.STD\_LOGIC\_UNSIGNED.ALL;  entity RAM is  port( CLOCK : STD\_LOGIC;  WR : IN STD\_LOGIC;  ADDR\_BUS : IN STD\_LOGIC\_VECTOR(1 DOWNTO 0);  IN\_DATA\_BUS : IN STD\_LOGIC\_VECTOR(7 DOWNTO 0);  OUT\_DATA\_BUS : OUT STD\_LOGIC\_VECTOR(7 DOWNTO 0));  end RAM;  architecture RAM\_arch of RAM is  type ram\_type is array (3 downto 0) of STD\_LOGIC\_VECTOR(7 downto 0);  signal UNIT : ram\_type;  begin  process(CLOCK, ADDR\_BUS, UNIT)  begin  if (rising\_edge(CLOCK)) then  if (WR = '1') then  UNIT(conv\_integer(ADDR\_BUS)) <= IN\_DATA\_BUS;  end if;  end if;  OUT\_DATA\_BUS <= UNIT(conv\_integer(ADDR\_BUS));  end process;  end RAM\_arch; |


|  |
| --- |
| Файл SEG\_DECODER.vhd  library IEEE;  use IEEE.STD\_LOGIC\_1164.ALL;  use IEEE.STD\_LOGIC\_ARITH.ALL;  use IEEE.STD\_LOGIC\_UNSIGNED.ALL;  entity BIN\_TO\_BCD is  port( CLOCK : IN STD\_LOGIC;  RESET : IN STD\_LOGIC;  ACC\_DATA\_OUT\_BUS : IN STD\_LOGIC\_VECTOR(7 DOWNTO 0);  COMM\_ONES : OUT STD\_LOGIC;  COMM\_DECS : OUT STD\_LOGIC;  COMM\_HUNDREDS : OUT STD\_LOGIC;  SEG\_A : OUT STD\_LOGIC;  SEG\_B : OUT STD\_LOGIC;  SEG\_C : OUT STD\_LOGIC;  SEG\_D : OUT STD\_LOGIC;  SEG\_E : OUT STD\_LOGIC;  SEG\_F : OUT STD\_LOGIC;  SEG\_G : OUT STD\_LOGIC;  DP : OUT STD\_LOGIC);  end BIN\_TO\_BCD;  architecture Behavioral of BIN\_TO\_BCD is  signal ONES\_BUS : STD\_LOGIC\_VECTOR(3 downto 0) := "0000";  signal DECS\_BUS : STD\_LOGIC\_VECTOR(3 downto 0) := "0001";  signal HONDREDS\_BUS : STD\_LOGIC\_VECTOR(3 downto 0) := "0000";  begin  BIN\_TO\_BCD : process (ACC\_DATA\_OUT\_BUS)  variable hex\_src : STD\_LOGIC\_VECTOR(7 downto 0) ;  variable bcd : STD\_LOGIC\_VECTOR(11 downto 0) ;  begin  bcd := (others => '0') ;  hex\_src := ACC\_DATA\_OUT\_BUS;  for i in hex\_src'range loop  if bcd(3 downto 0) > "0100" then  bcd(3 downto 0) := bcd(3 downto 0) + "0011" ;  end if ;  if bcd(7 downto 4) > "0100" then  bcd(7 downto 4) := bcd(7 downto 4) + "0011" ;  end if ;  if bcd(11 downto 8) > "0100" then  bcd(11 downto 8) := bcd(11 downto 8) + "0011" ;  end if ;    bcd := bcd(10 downto 0) & hex\_src(hex\_src'left) ; -- shift bcd + 1 new entry  hex\_src := hex\_src(hex\_src'left - 1 downto hex\_src'right) & '0' ; -- shift src + pad with 0  end loop ;  HONDREDS\_BUS <= bcd (11 downto 8);  DECS\_BUS <= bcd (7 downto 4);  ONES\_BUS <= bcd (3 downto 0);    end process BIN\_TO\_BCD;    INDICATE : process(CLOCK)  type DIGIT\_TYPE is (ONES, DECS, HUNDREDS);    variable CUR\_DIGIT : DIGIT\_TYPE := ONES;  variable DIGIT\_VAL : STD\_LOGIC\_VECTOR(3 downto 0) := "0000";  variable DIGIT\_CTRL : STD\_LOGIC\_VECTOR(6 downto 0) := "0000000";  variable COMMONS\_CTRL : STD\_LOGIC\_VECTOR(2 downto 0) := "000";    begin  if (rising\_edge(CLOCK)) then  if(RESET = '0') then  case CUR\_DIGIT is  when ONES =>  DIGIT\_VAL := ONES\_BUS;  CUR\_DIGIT := DECS;  COMMONS\_CTRL := "001";  when DECS =>  DIGIT\_VAL := DECS\_BUS;  CUR\_DIGIT := HUNDREDS;  COMMONS\_CTRL := "010";  when HUNDREDS =>  DIGIT\_VAL := HONDREDS\_BUS;  CUR\_DIGIT := ONES;  COMMONS\_CTRL := "100";  when others =>  DIGIT\_VAL := ONES\_BUS;  CUR\_DIGIT := ONES;  COMMONS\_CTRL := "000";  end case;    case DIGIT\_VAL is --abcdefg  when "0000" => DIGIT\_CTRL := "1111110";  when "0001" => DIGIT\_CTRL := "0110000";  when "0010" => DIGIT\_CTRL := "1101101";  when "0011" => DIGIT\_CTRL := "1111001";  when "0100" => DIGIT\_CTRL := "0110011";  when "0101" => DIGIT\_CTRL := "1011011";  when "0110" => DIGIT\_CTRL := "1011111";  when "0111" => DIGIT\_CTRL := "1110000";  when "1000" => DIGIT\_CTRL := "1111111";  when "1001" => DIGIT\_CTRL := "1111011";  when others => DIGIT\_CTRL := "0000000";  end case;  else  DIGIT\_VAL := ONES\_BUS;  CUR\_DIGIT := ONES;  COMMONS\_CTRL := "000";  end if;    COMM\_ONES <= COMMONS\_CTRL(0);  COMM\_DECS <= COMMONS\_CTRL(1);  COMM\_HUNDREDS <= COMMONS\_CTRL(2);    SEG\_A <= DIGIT\_CTRL(6);  SEG\_B <= DIGIT\_CTRL(5);  SEG\_C <= DIGIT\_CTRL(4);  SEG\_D <= DIGIT\_CTRL(3);  SEG\_E <= DIGIT\_CTRL(2);  SEG\_F <= DIGIT\_CTRL(1);  SEG\_G <= DIGIT\_CTRL(0);  DP <= '0';    end if;  end process INDICATE;  end Behavioral; |




*Рис. 2 – Часова діаграма ACC*

**


*Рис. 3 – Часова діаграма ALU*

**


*Рис. 4 – Часова діаграма MUX*

**

*Рис. 5 – Часова діаграма RAM*


**

*Рис 6. – Часова діграма SEG\_DECODER*

**

*Рис 7. – Часова діграма TopLevel*

|  |
| --- |
| *Файл TopLevelTest.vhd*  *-- \* Test Bench - User Defined Section \**  *tb : PROCESS*  *BEGIN*    *lp1: for i in 4 to 4 loop*  *lp2: for j in 1 to 1 loop*  *ENTER\_OP1 <= '1';*  *ENTER\_OP2 <= '1';*  *CALCULATE <= '1';*  *case(std\_logic\_vector(to\_unsigned(i, 8))) is*  *when x"00" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 0);*  *when x"01" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 1);*  *when x"02" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 2);*  *when x"03" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 3);*  *when x"04" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 4);*  *when x"05" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 5);*  *when x"06" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 6);*  *when x"07" =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 7);*  *when others =>*  *TEST <= std\_logic\_vector(signed(std\_logic\_vector(unsigned(std\_logic\_vector(to\_unsigned(to\_integer(unsigned(std\_logic\_vector(to\_unsigned(i, 8)))) + to\_integer(unsigned(std\_logic\_vector(to\_unsigned(j, 8)))) + 10, 8)))) AND std\_logic\_vector(to\_unsigned(j, 8))) SLL 0);*  *end case;*  *DATA\_IN <= (others => '0');*  *RESET <= '0';*  *wait for CLKP;*  *RESET <= '1';*  *wait for CLKP;*  *DATA\_IN <= (std\_logic\_vector(to\_unsigned(i, 8))); -- A*  *ENTER\_OP1 <= '0';*  *wait for CLKP;*  *ENTER\_OP1 <= '1';*  *wait for CLKP \* 2;*  *DATA\_IN <= (std\_logic\_vector(to\_unsigned(j, 8))); -- B*  *ENTER\_OP2 <= '0';*  *wait for CLKP;*  *ENTER\_OP2 <= '1';*  *wait for CLKP \* 2;*  *CALCULATE <= '0'; -- START CALCULATION*  *REPORT "OP1 = (" & integer'image(i) & ") and OP2 = (" & integer'image(j) & ") calculation started" SEVERITY NOTE;*  *wait for CLKP \* 7;*  *assert ACC\_OUT\_BUS = TEST severity FAILURE;*  *REPORT "OP1 = (" & integer'image(i) & ") and OP2 = (" & integer'image(j) & ") calculation finished" SEVERITY NOTE;*  *wait for CLKP;*  *end loop;*  *end loop;*  *WAIT; -- will wait forever*  *END PROCESS;*  *-- \*\*\* End Test Bench - User Defined Section \*\*\**  *END;* |



*Рис.9 – Успішна прошивка*

**Висновок:** Виконуючи дану лабораторну роботу я навчився реалізовувати цифровий автомат для обчислення значення виразів використовуючи засоби VHDL.